Rancid (Really Awesome New Cisco confIg Differ)

Podemos utilizar Rancid para hacer backup de las configuraciones de nuestros routers, switches o firewalls Debian 8 rancid

Dispositivo	Descripción
alteon	Alteon WebOS switches.
baynet	Bay Networks router.
cat5	Cisco catalyst series 5000 and 4000 switches (i.e.: running the catalyst OS, not IOS).
ciscoCisco router, PIX, or switch such as the 3500XL or 6000 running IOS (or IOS-like) OS.
css	Cisco content services switch.
enterasys	An enterasys NAS. This is currently an alias for the riverstone device type.
erx	A Juniper E-series edge router.
Extreme	An Extreme switch.
ezt3	An ADC-Kentrox EZ-T3 mux.
force10	A Force10 router.
fortigate	Equipos Fortigate
foundry	A Foundry router, switch, or router-switch. This includes HP Procurve switches that are OEMs of Foundry products, such as the HP9304M.
hitachi	A Hitachi routers.
h3c	3Com SuperStack 4, H3C, HP Networking ('A' & some 'E' portfolio, post 2010 3Com acquitision), some Huawei equipment.
hp	A HP Procurve switch such as the 2524 or 4108 procurve switches. Also see the foundry type.
mrtd	A host running the (merit) MRTd daemon.
netscalar	A Netscalar load balancer.
netscreen	A Netscreen firewall.
redback	A Redback router, NAS, etc.
tnt	A lucent TNT.
zebra	Zebra routing software.
riverstone	A Riverstone NAS or Cabletron (starting with version ~9.0.3) router.
juniper	A Juniper router.

Ritio oficial : http://www.shrubbery.net/rancid/

Agregado para soporte H3C : https://sites.google.com/site/jrbinks/code/rancid/h3c