3COM

5500 Series

Configuración Minicom

pu port /dev/ttyUSB0 pu baudrate 19200 pu bits 8 pu parity N pu stopbits 1 pu hasdcd No pu rtscts No pu xonxoff No

Ejemplo de pantalla de booteo

Starting......
******************************************************************
* *
* SuperStack 4 Switch 5500G-EI 24-Port BOOTROM, Version 4.03 *
* *
******************************************************************
Copyright (c) 2004-2007 3Com Corporation and its licensors.
Creation date : Jan 23 2007, 11:19:21
CPU type : BCM1122
CPU Clock Speed : 400MHz
BUS Clock Speed : 33MHz
Memory Size : 128MB
Mac Address : 0022573c6480
Press Ctrl-B to enter Boot Menu... 0
Auto-booting...
Decompress Image....................................................................!
Starting at 0x80020000...
Press Ctrl-B to enter Boot Menu... 1
password:
BOOT MENU
1. Download application file to flash
2. Select application file to boot
3. Display all files in flash
4. Delete file from flash
5. Modify bootrom password
6. Enter bootrom upgrade menu
7. Skip current configuration file
8. Set bootrom password recovery
9. Set switch startup mode
0. Reboot
Enter your choice(0-9):